Firmware:
For TOTOLINK X5000R.

Change log:
1. X5000R transition version, support on the standard version, page upgrade to EasyMesh version;
Or you can directly use the special upgrade method (reset pending upgrade, refer to the attached documentation).

Standard version→EasyMesh version》》》OK
EasyMesh version→Standard version》》》NG.
The latest standard version: TOTOLINK_C8343R-1C_X5000R_IP04433_MT7621A_SPI_16M256M_V9.1.0u.6118_B20201102_ALL
The latest EasyMesh version: CS_C8344R_X5000R_IP04433_MT7621MT7915_SPI_16M256M_V9.1.0cu.2089_B20211224_ALL
To Upgrade:


To prevent upgrade failures, please read the following before proceeding with the upgrade process
1. Please verify the hardware version of your device for the firmware version. Wrong firmware upgrade may damage your device and void the warranty. 
For example, if your hardware yersion is V1.1 or V1x(=1.2.3. 4.), please download V1 version, V2 version is not for your device.
2. DO NOT power off the device or close the browser window during the upload because it may crash the system.
3. The correct upgrade firmware is a file suffixed with the Web.